//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//




.Set READY_VAR = 02
Command ID:	WORK_MODE_DUPLEX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Command:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 80
Receive	Command:84 A9 61 00 02 00 1A 00
Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 04 03 
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 03 30 26 01 03
Pause 2000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 03 30 26 05 03
Pause 500
Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 02 03 
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 03 30 26 01 03
Pause 2000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
PAUSE 500
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 03 30 26 03 03
Pause 500
Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 09 00 26 04 ff 03 b4 00 cb 07 0b 
//Send	Command: 84 A9 61 00 03 00 26 04 03
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 05 30 26 01 ff 03 b4 
//Receive	Command: 84 A9 61 00 03 30 26 01 03
Pause 2000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
PAUSE 500
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 05 30 26 05 ff 03 b4 
//Receive	Command: 84 A9 61 00 03 30 26 05 03


// 
Command ID:	WORK_MODE_IDLE
Send	Command: 84 A9 61 00 04 00 18 00 00 00
Receive	Command:84 A9 61 00 02 00 18 00

Command ID:	WORK_MODE_DUPLEX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Command:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 80
Receive	Command:84 A9 61 00 02 00 1A 00
Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 80 07
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 03 30 26 81 07
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 03 30 26 80 07
PAUSE 1000
////////////
Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 84 09
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00
Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 03 30 26 81 09
PAUSE 1000
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
PAUSE 1000
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 03 30 26 85 09

Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 94 13
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00

Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 03 30 26 91 13

Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
PAUSE 1000
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 03 30 26 95 13

Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 c4 64
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00

Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 03 30 26 c1 64
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
PAUSE 1000
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 03 30 26 c5 64

Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 a4 18
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 01
Receive	Command:84 A9 61 00 02 00 19 00

Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 03 30 26 a1 18
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
PAUSE 1000
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 03 30 26 a5 18
PAUSE 1000

Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 03 00 26 88 21
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00

Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 1000
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 03 30 26 89 21
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
PAUSE 1000
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 03 30 26 88 21


Command ID:	SUB_AUDIO
Send	Command: 84 A9 61 00 05 00 26 a4 ff 00 17 
Receive	Command:84 A9 61 00 02 00 26 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 00 19 {READY_VAR}
Receive	Command:84 A9 61 00 02 00 19 00

Command ID:	CALL_START
Send	Command: 84 A9 61 00 01 05 78
PAUSE 500
Receive	Command:84 A9 61 00 02 05 78 00
Receive	Command:84 A9 61 00 05 30 26 a1 ff 00 17 
Command ID:	CALL_END
Send	Command: 84 A9 61 00 01 00 21 
PAUSE 1000
Receive	Command:84 A9 61 00 02 00 21 00
Receive	Command:84 A9 61 00 05 30 26 a5 ff 00 17 
