//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//

.Set READY_VAR = 01
Command ID:	VOCODER_SEL
Send	Command: 84 A9 61 00 02 00 10 03
 Receive	Data:84 A9 61 00 02 00 10 00
pause 4000
Command ID:	VOCODER_CMODE
Send	Command: 84 A9 61 00 02 00 02 0A
Receive	Data:84 A9 61 00 02 00 02 00


Command ID:	NXDN_CALL_OPTION
Send	Command: 84 A9 61 00 06 06 47 82 00 00 00 00
Receive Data:   84 A9 61 00 02 06 47 00
Pause 1000
Command ID:	WORK_MODE_DUPLEX
Send	Command: 84 A9 61 00 04 00 18 03 00 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 02
Receive	Data:84 A9 61 00 02 00 1A 00
Command ID:	CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 01
Receive	Data:84 A9 61 00 02 03 19 00

Pause 1000
Command ID:	NXDN_DATA_FRAME
Send command: 84 a9 61 00 13 00 43 00 00 0f 10 81 00 00 00 20 03 88 93 90 00 00 00 00 00
Receive Data: 84 a9 61 00 01 20 43

Command ID:   NXDN_DATA_FRAME
Send command: 84 a9 61 00 09 00 43 00 00 05 8C 81 00 00 00
Receive Data: 84 a9 61 00 01 20 43


 Receive	Data:84 A9 61 00 13 20 43 E0 00 0F 10 81 00 00 00 20 03 88 93 90 00 00 00 00 00
Receive	Data:84 A9 61 00 09 20 43 C0 00 05 8C 81 00 00 00


PAUSE 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 80 F3
Receive	Data:84 A9 61 00 04 30 08 03 80 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 81 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 81 F3
Receive	Data:84 A9 61 00 04 30 08 03 81 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 81 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 82 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 82 F3
Receive	Data:84 A9 61 00 04 30 08 03 82 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 82 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 83 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 83 F3
Receive	Data:84 A9 61 00 04 30 08 03 83 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 83 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 84 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 84 F3
Receive	Data:84 A9 61 00 04 30 08 03 84 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 84 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 85 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 85 F3
Receive	Data:84 A9 61 00 04 30 08 03 85 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 85 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 86 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 86 F3
Receive	Data:84 A9 61 00 04 30 08 03 86 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 86 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 87 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 87 F3
Receive	Data:84 A9 61 00 04 30 08 03 87 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 87 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 88 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 88 F3
Receive	Data:84 A9 61 00 04 30 08 03 88 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 88 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 89 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 89 F3
Receive	Data:84 A9 61 00 04 30 08 03 89 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 89 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8A F3
Receive	Data:84 A9 61 00 04 30 08 03 8A F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8B F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8B F3
Receive	Data:84 A9 61 00 04 30 08 03 8B F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8B F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8C F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8C F3
Receive	Data:84 A9 61 00 04 30 08 03 8C F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8C F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8D F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8D F3
Receive	Data:84 A9 61 00 04 30 08 03 8D F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8D F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8E F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8E F3
Receive	Data:84 A9 61 00 04 30 08 03 8E F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8E F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 8F F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 8F F3
Receive	Data:84 A9 61 00 04 30 08 03 8F F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 8F F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000



Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 20 F3
Receive	Data:84 A9 61 00 04 30 08 03 20 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 05 F3
Receive	Data:84 A9 61 00 04 30 08 03 05 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 0A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 0A F3
Receive	Data:84 A9 61 00 04 30 08 03 0A F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 0A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 10 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 10 F3
Receive	Data:84 A9 61 00 04 30 08 03 10 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 10 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 20 F3
Receive	Data:84 A9 61 00 04 30 08 03 20 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 30 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 30 F3
Receive	Data:84 A9 61 00 04 30 08 03 30 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 30 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 40 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 40 F3
Receive	Data:84 A9 61 00 04 30 08 03 40 F4
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 40 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 50 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 50 F3
Receive	Data:84 A9 61 00 04 30 08 03 50 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 50 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 60 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 60 F3
Receive	Data:84 A9 61 00 04 30 08 03 60 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 60 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 70 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 70 F3
Receive	Data:84 A9 61 00 04 30 08 03 70 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 70 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 7A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 7A F3
Receive	Data:84 A9 61 00 04 30 08 03 7A F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7A F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 80 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 80 D0
Receive	Data:84 A9 61 00 04 30 08 03 80 D0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 20 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 20 D0
Receive	Data:84 A9 61 00 04 30 08 03 20 D0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 05 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 05 D0
Receive	Data:84 A9 61 00 04 30 08 03 05 D0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 03 7A D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 7A D0
Receive	Data:84 A9 61 00 04 30 08 03 7A D0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7A D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 20 08 01 FF A6
Receive	Data:84 A9 61 00 04 30 08 03 FF A6

pause 4000

Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 80 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 20 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 05 F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 7a F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 7A F3
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7a F3
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 80 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 80 D0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 80 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 20 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 20 D0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 20 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 05 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 05 D0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 05 D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 01 7a D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 7A D0
pause 1000
Command ID:	VOCODER_TONE
Send	Command: 84 A9 61 00 04 00 08 00 7a D0
Receive	Data:84 A9 61 00 02 00 08 00
Receive	Data:84 A9 61 00 04 30 08 03 FF A6
pause 1000


Command ID: NXDN_DATA_FRAME
Send command: 84 a9 61 00 09 00 43 c0 00 05 94 9e 00 00 00 

Receive       Data:84 a9 61 00 01 20 43

Receive	Data:84 A9 61 00 02 20 17 0A

Pause 500
Command ID: CARRIER_LOST
Send command: 84 A9 61 00 02 00 19 00
Receive Data: 84 A9 61 00 02 00 19 00

